
Carpentry and Joinery portable power tools

# Crossword



**Across**

2. Other than nails, this is another type of fixing used to secure plasterboards (6)

3. Many years ago this nail was used to secure flooring to joists (3-5)

7. This type of nail is used on structural carcassing such as stud partitions (5-4)

8. The hole drilled prior to inserting a screw is known as a \_\_\_\_\_\_\_\_\_\_\_ hole (5)

9. Nails and screws are best processed in this way if they are used externally (10)

10. The fixings used to secure materials to plasterboard are called hollow wall \_\_\_\_\_\_\_\_\_\_\_ (7)

**Down**

1. This type of nail is used to secure skirting boards (4-4)

4. The three head types on screws are pozi, Phillips and \_\_\_\_\_\_\_\_\_\_\_ (7)

5. When inserting screws into masonry products, this fixing aid is required (4-4)

6. This type of nail has a series of ridges on it to secure it to the surface material (7-4)